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Case - Dead working
Video link: 

· English https://youtu.be/D2FbzcGe5T0
· Spanish https://youtu.be/1ny9DwKeO44  

· Maltese https://youtu.be/3vupLqaC6l0
· Danish https://www.youtube.com/embed/KN9q9mzZiZg?start=456&end=640 
· Greek https://youtu.be/S4HlecyIQjM
Teacher instruction:

The case is based on watching a video which deals with safety issues:

The video can be watched with Danish or English dialogue. The English video can be watched with subtitles in Greek, Maltese, and Spanish

Read through the suggested Questions and Answers and ensure that all participants know what to look for

Let the course participants watch the video (Approx. 3 minutes), either together or individually. 

Question

Q1: Name some of the safety steps that are needed when you have chosen to work on a dead installation

Q2: What should you do before removing a fuse link?

Q3: It is important to ensure that the installation is dead, but why is the old type voltage indicator unsuitable for this?

Answer

A1: Switch off using the disconnector, lock the disconnector using a padlock, hang up a sign so it is evident that the power must not be reconnected.

A2: Wear safety glasses and use an insulated fuse remover

A3: The long uninsulated tip increases the risk of creating a short circuit and thus an arc.
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